{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["附件 (2)"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"附件 (2)","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"merged":[[0,0,0,2],[1,0,1,7],[3,7,11,7],[12,2,12,5],[13,2,13,5],[14,0,14,1],[14,2,14,5]],"flags":["formulas_cached_only"]}
["附件1："]
["网络路由器明细表"]
["序号","分项名称","参考品牌","规格型号","单位","技术要求","数量","备注"]
[1,"核心路由器","H3C","RT-SR6602-X1","台","(4GE Combo,1 FIP 插槽)",1,"图书馆网络总控室"]
[2,"光口接口模块","H3C","RT-HIM-8GBP-H3","台","4端口千兆以太网光口接口模块(SFP)",1]
[3,"灵活接口平台",null,"RT-FIP-20","台","2 HIM 插槽",1]
[4,"电源模块","H3C","LSWM1AC300","台","300W交流系统电源模块",1]
[5,"电口模块","H3C","SFP-GE-T","块",null,3]
[6,"单模模块","H3C","SFP-GE-LX-SM1310-A","块","SFP封装，波长1310nm，传输40KM以上",1]
[7,"单模光纤跳线","quickenet","LC--LC","条","4M",4]
[8,"单模光纤跳线","quickenet","SC--LC","条","4M",4]
[9,"超六类网线","SIMON(西蒙)","RJ45*2","条","3M",10]
[10,"技术服务费","    现有网络核心交换机、路由器配置备份，路由器连接的断开，路由重新选路，三角形路由结构部署，三角形路由配置的编写，接入带宽路由策略的调整与优化",{"$nulls":3},1]
[11,"安装调试费","   网络总控核心交换机线路的测试与查找，网络总控路由设备线路的测试与查找，光纤跳线的部署，三角形路由结构部署，交换路由连接部署",{"$nulls":3},1]
["合计"]